# Protocol Compliance List

OpenGGSN supports both GTP0 (GSM 09.60) and GTP1 (3GPP 29.060). In the following tables the support of each individual message type is detailed. The numbers before each feature indicates the relevant section in the standard.

## GSM 09.60 (GTPv0)

Feature | gtplib | ggsn | sgsnemu | notes
7.4 Path Management Messages |  |  |  |
7.4.1 Echo Request | Supported | Supported | Supported |
7.4.2 Echo Response | Supported | Supported | Supported |
7.4.3 Version Not Supported | Supported | Supported | Supported |
7.5 Tunnel Management Messages |  |  |  |
7.5.1 Create PDP Context Request | Supported | Supported | Supported |
7.5.2 Create PDP Context Response | Supported | Supported | Supported |
7.5.3 Update PDP Context Request | Supported | Supported | Not applicable |
7.5.4 Update PDP Context Response | Supported | Supported | Not applicable |
7.5.5 Delete PDP Context Request | Supported | Supported | Supported |
7.5.6 Delete PDP Context Response | Supported | Supported | Supported |
7.5.7 Create AA PDP Context Request | Unsupported | Unsupported | Unsupported |
7.5.8 Create AA PDP Context Response | Unsupported | Unsupported | Unsupported |
7.5.9 Delete AA PDP Context Request | Unsupported | Unsupported | Unsupported |
7.5.10 Delete AA PDP Context Response | Unsupported | Unsupported | Unsupported |
7.5.11 Error Indication | Supported | Supported | Supported |
7.5.12 PDU Notification Request | Unsupported | Unsupported | Unsupported |
7.5.13 PDU Notification Response | Unsupported | Unsupported | Unsupported |
7.5.14 PDU Notification Reject Request | Unsupported | Unsupported | Unsupported |
7.5.15 PDU Notification Reject Response | Unsupported | Unsupported | Unsupported |
7.6 Location Management Messages |  |  |  |
7.6.1 Send Routeing Information for GPRS Request | Unsupported | Unsupported | Not applicable |
7.6.2 Send Routeing Information for GPRS Response | Unsupported | Unsupported | Not applicable |
7.6.3 Failure Report Request | Unsupported | Unsupported | Not applicable |
7.6.3 Failure Report Response | Unsupported | Unsupported | Not applicable |
7.6.5 Note MS GPRS Present Request | Unsupported | Unsupported | Not applicable |
7.6.6 Note MS GPRS Present Response | Unsupported | Unsupported | Not applicable |
7.5 Mobility Management Messages |  |  |  |
7.5.1 Identification Request | Unsupported | Not applicable | Not applicable |
7.5.2 Identification Response | Unsupported | Not applicable | Not applicable |
7.5.3 SGSN Context Request | Unsupported | Not applicable | Not applicable |
7.5.4 SGSN Context Response | Unsupported | Not applicable | Not applicable |
7.5.5 SGSN Context Acknowledge | Unsupported | Not applicable | Not applicable |

## 3GPP 29.060 (GTPv1)

Feature | gtplib | ggsn | sgsnemu | notes
7.2 Path Management Messages |  |  |  |
7.2.1 Echo Request | Supported | Supported | Supported |
7.2.2 Echo Response | Supported | Supported | Supported |
7.2.3 Version Not Supported | Supported | Supported | Supported |
7.2.4 Supported Extension Headers Notification | Supported | Supported | Supported |
7.3 Tunnel Management Messages |  |  |  |
7.3.1 Create PDP Context Request | Supported | Supported | Supported | 1
7.3.2 Create PDP Context Response | Supported | Supported | Supported |
7.3.3 Update PDP Context Request | Supported | Supported | Not applicable | 1
7.3.4 Update PDP Context Response | Supported | Supported | Not applicable |
7.3.5 Delete PDP Context Request | Supported | Supported | Supported |
7.3.6 Delete PDP Context Response | Supported | Supported | Supported |
7.3.7 Error Indication | Supported | Supported | Supported |
7.3.8 PDU Notification Request | Unsupported | Unsupported | Unsupported |
7.3.9 PDU Notification Response | Unsupported | Unsupported | Unsupported |
7.3.10 PDU Notification Reject Request | Unsupported | Unsupported | Unsupported |
7.3.10 PDU Notification Reject Response | Unsupported | Unsupported | Unsupported |
7.4 Location Management Messages |  |  |  |
7.4.1 Send Routeing Information for GPRS Request | Unsupported | Unsupported | Not applicable |
7.4.2 Send Routeing Information for GPRS Response | Unsupported | Unsupported | Not applicable |
7.4.3 Failure Report Request | Unsupported | Unsupported | Not applicable |
7.4.3 Failure Report Response | Unsupported | Unsupported | Not applicable |
7.4.5 Note MS GPRS Present Request | Unsupported | Unsupported | Not applicable |
7.4.6 Note MS GPRS Present Response | Unsupported | Unsupported | Not applicable |
7.5 Mobility Management Messages |  |  |  |
7.5.1 Identification Request | Unsupported | Not applicable | Not applicable |
7.5.2 Identification Response | Unsupported | Not applicable | Not applicable |
7.5.3 SGSN Context Request | Unsupported | Not applicable | Not applicable |
7.5.4 SGSN Context Response | Unsupported | Not applicable | Not applicable |
7.5.5 SGSN Context Acknowledge | Unsupported | Not applicable | Not applicable |
7.5.6 Forward Relocation Request | Unsupported | Not applicable | Not applicable |
7.5.7 Forward Relocation Response | Unsupported | Not applicable | Not applicable |
7.5.8 Forward Relocation Complete | Unsupported | Not applicable | Not applicable |
7.5.9 Relocation Cancel Request | Unsupported | Not applicable | Not applicable |
7.5.10 Relocation Cancel Response | Unsupported | Not applicable | Not applicable |
7.5.11 Forward Relocation Complete Acknowledge | Unsupported | Not applicable | Not applicable |
7.5.12 Forward SRNS Context Acknowledge | Unsupported | Not applicable | Not applicable |
7.5.13 Forward SRNS Context | Unsupported | Not applicable | Not applicable |

## Notes

1) The "Secondary PDP Context Activation Procedure" is not supported.